| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5614: Machine instructions VSUBB VSUBW VSUBD VSUBQ

Tested procedures
  IizVPSUBB IizVPSUBW IizVPSUBD IizVPSUBQ

Source & expected listing t5614.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5614 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C5E9F8CB | VPSUBB XMM1,XMM2,XMM3 |00000004:C5EDF8CB | VPSUBB YMM1,YMM2,YMM3 |00000008:62F16D0CF8CB | VPSUBB XMM1,XMM2,XMM3,MASK=K4 |0000000E:62F16DACF8CB | VPSUBB YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |00000014:62F16DCCF8CB | VPSUBB ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |0000001A:C5E9F84D40 | VPSUBB XMM1,XMM2,[RBP+40h] |0000001F:C5EDF84D40 | VPSUBB YMM1,YMM2,[RBP+40h] |00000024:62F16D48F84D01<6 | VPSUBB ZMM1,ZMM2,[RBP+40h] |0000002B:62F16D0CF84D04<4 | VPSUBB XMM1,XMM2,[RBP+40h],MASK=K4 |00000032:62F16DCCF84D01<6 | VPSUBB ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000039:C5E9F9CB | VPSUBW XMM1,XMM2,XMM3 |0000003D:C5EDF9CB | VPSUBW YMM1,YMM2,YMM3 |00000041:62F16D0CF9CB | VPSUBW XMM1,XMM2,XMM3,MASK=K4 |00000047:62F16DACF9CB | VPSUBW YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |0000004D:62F16DCCF9CB | VPSUBW ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000053:C5E9F94D40 | VPSUBW XMM1,XMM2,[RBP+40h] |00000058:C5EDF94D40 | VPSUBW YMM1,YMM2,[RBP+40h] |0000005D:62F16D48F94D01<6 | VPSUBW ZMM1,ZMM2,[RBP+40h] |00000064:62F16D0CF94D04<4 | VPSUBW XMM1,XMM2,[RBP+40h],MASK=K4 |0000006B:62F16DACF94D02<5 | VPSUBW YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000072:62F16DCCF94D01<6 | VPSUBW ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000079:C5E9FACB | VPSUBD XMM1,XMM2,XMM3 |0000007D:C5EDFACB | VPSUBD YMM1,YMM2,YMM3 |00000081:62F16D0CFACB | VPSUBD XMM1,XMM2,XMM3,MASK=K4 |00000087:62F16DACFACB | VPSUBD YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |0000008D:62F16DCCFACB | VPSUBD ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000093:62F16928FACB | VPSUBD ZMM1,ZMM2,ZMM3,EH=0,OPER=2 ; MVEX swizzle {badc}. |00000099:C5E9FA4D40 | VPSUBD XMM1,XMM2,[RBP+40h] |0000009E:C5EDFA4D40 | VPSUBD YMM1,YMM2,[RBP+40h] |000000A3:62F16D48FA4D01<6 | VPSUBD ZMM1,ZMM2,[RBP+40h] |000000AA:62F16D18FA4D10<2 | VPSUBD XMM1,XMM2,[RBP+40h],BCST=ON |000000B1:62F16D38FA4D10<2 | VPSUBD YMM1,YMM2,[RBP+40h],BCST=ON |000000B8:62F16D58FA4D10<2 | VPSUBD ZMM1,ZMM2,[RBP+40h],BCST=ON |000000BF:62F16D0CFA4D04<4 | VPSUBD XMM1,XMM2,[RBP+40h],MASK=K4 |000000C6:62F16D1CFA4D10<2 | VPSUBD XMM1,XMM2,[RBP+40h],MASK=K4,BCST=ON |000000CD:62F16DBCFA4D10<2 | VPSUBD YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |000000D4:62F16DCCFA4D01<6 | VPSUBD ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |000000DB:62F16908FA4D01<6 | VPSUBD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=0 ; {16to16}. |000000E2:62F16918FA4D10<2 | VPSUBD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=1 ; {1to16}. |000000E9:62F16928FA4D04<4 | VPSUBD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=2 ; {4to16}. |000000F0:62F16948FA4D04<4 | VPSUBD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=4 ; {uint8}. |000000F7:C5E9FBCB | VPSUBQ XMM1,XMM2,XMM3 |000000FB:C5EDFBCB | VPSUBQ YMM1,YMM2,YMM3 |000000FF:62F1EDACFBCB | VPSUBQ YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |00000105:62F1EDACFBCB | VPSUBQ YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |0000010B:62F1EDCCFBCB | VPSUBQ ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000111:C5E9FB4D40 | VPSUBQ XMM1,XMM2,[RBP+40h] |00000116:C5EDFB4D40 | VPSUBQ YMM1,YMM2,[RBP+40h] |0000011B:62F1ED48FB4D01<6 | VPSUBQ ZMM1,ZMM2,[RBP+40h] |00000122:62F1ED18FB4D08<3 | VPSUBQ XMM1,XMM2,[RBP+40h],BCST=ON |00000129:62F1ED38FB4D08<3 | VPSUBQ YMM1,YMM2,[RBP+40h],BCST=ON |00000130:62F1ED58FB4D08<3 | VPSUBQ ZMM1,ZMM2,[RBP+40h],BCST=ON |00000137:62F1ED0CFB4D04<4 | VPSUBQ XMM1,XMM2,[RBP+40h],MASK=K4 |0000013E:62F1ED1CFB4D08<3 | VPSUBQ XMM1,XMM2,[RBP+40h],MASK=K4,BCST=ON |00000145:62F1EDBCFB4D08<3 | VPSUBQ YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |0000014C:62F1EDCCFB4D01<6 | VPSUBQ ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON | |ENDPROGRAM t5614`

Expected messages t5614.out
  `I0180 Assembling source file "t5614.htm". I0270 Assembling source "t5614". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5614". "t5614.htm"{58} I0510 Assembling program pass 1. "t5614.htm"{58} I0530 Assembling program pass 2 - final. "t5614.htm"{58} I0660 16bit TINY BIN file "t5614.bin" created, size=339. "t5614.htm"{116} I0650 Program "t5614" assembled in 2 passes with errorlevel 0. "t5614.htm"{116} I0750 Source "t5614" (134 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5614.htm.lst" created, size=4119. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲