| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4650: Machine instructions VFMADDPS VFMADDPD VFMADDSUBPS VFMADDSUBPD

Tested procedures
  IiaVFMADDPS IiaVFMADDPD IiaVFMADDSUBPS IiaVFMADDSUBPD

Source & expected listing t4650.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=24,CPU=X64,SIMD=AVX,FMA=ON,AMD=ON | |t4650 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C4E369680E40 | VFMADDPS XMM1,XMM2,[RSI],XMM4 |00000006:C4E369690E40 | VFMADDPD XMM1,XMM2,[RSI],XMM4 |0000000C:C4E3695C0E40 | VFMADDSUBPS XMM1,XMM2,[RSI],XMM4 |00000012:C4E3695D0E40 | VFMADDSUBPD XMM1,XMM2,[RSI],XMM4 |00000018:C4E3E9680E30 | VFMADDPS XMM1,XMM2,XMM3,[RSI] |0000001E:C4E3E9690E30 | VFMADDPD XMM1,XMM2,XMM3,[RSI] |00000024:C4E3E95C0E30 | VFMADDSUBPS XMM1,XMM2,XMM3,[RSI] |0000002A:C4E3E95D0E30 | VFMADDSUBPD XMM1,XMM2,XMM3,[RSI] |00000030:C4E36968CB40 | VFMADDPS XMM1,XMM2,XMM3,XMM4 |00000036:C4E36969CB40 | VFMADDPD XMM1,XMM2,XMM3,XMM4 |0000003C:C4E3695CCB40 | VFMADDSUBPS XMM1,XMM2,XMM3,XMM4 |00000042:C4E3695DCB40 | VFMADDSUBPD XMM1,XMM2,XMM3,XMM4 |00000048:C4E3E968CC30 | VFMADDPS XMM1,XMM2,XMM3,XMM4,CODE=LONG |0000004E:C4E3E969CC30 | VFMADDPD XMM1,XMM2,XMM3,XMM4,CODE=LONG |00000054:C4E3E95CCC30 | VFMADDSUBPS XMM1,XMM2,XMM3,XMM4,CODE=LONG |0000005A:C4E3E95DCC30 | VFMADDSUBPD XMM1,XMM2,XMM3,XMM4,CODE=LONG |00000060:C4E36D680E40 | VFMADDPS YMM1,YMM2,[RSI],YMM4 |00000066:C4E36D690E40 | VFMADDPD YMM1,YMM2,[RSI],YMM4 |0000006C:C4E36D5C0E40 | VFMADDSUBPS YMM1,YMM2,[RSI],YMM4 |00000072:C4E36D5D0E40 | VFMADDSUBPD YMM1,YMM2,[RSI],YMM4 |00000078:C4E3ED680E30 | VFMADDPS YMM1,YMM2,YMM3,[RSI] |0000007E:C4E3ED690E30 | VFMADDPD YMM1,YMM2,YMM3,[RSI] |00000084:C4E3ED5C0E30 | VFMADDSUBPS YMM1,YMM2,YMM3,[RSI] |0000008A:C4E3ED5D0E30 | VFMADDSUBPD YMM1,YMM2,YMM3,[RSI] |00000090:C4E36D68CB40 | VFMADDPS YMM1,YMM2,YMM3,YMM4 |00000096:C4E36D69CB40 | VFMADDPD YMM1,YMM2,YMM3,YMM4 |0000009C:C4E36D5CCB40 | VFMADDSUBPS YMM1,YMM2,YMM3,YMM4 |000000A2:C4E36D5DCB40 | VFMADDSUBPD YMM1,YMM2,YMM3,YMM4 |000000A8:C4E3ED68CC30 | VFMADDPS YMM1,YMM2,YMM3,YMM4,CODE=LONG |000000AE:C4E3ED69CC30 | VFMADDPD YMM1,YMM2,YMM3,YMM4,CODE=LONG |000000B4:C4E3ED5CCC30 | VFMADDSUBPS YMM1,YMM2,YMM3,YMM4,CODE=LONG |000000BA:C4E3ED5DCC30 | VFMADDSUBPD YMM1,YMM2,YMM3,YMM4,CODE=LONG | |ENDPROGRAM t4650`

Expected messages t4650.out
  `I0180 Assembling source file "t4650.htm". I0270 Assembling source "t4650". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4650". "t4650.htm"{58} I0510 Assembling program pass 1. "t4650.htm"{58} I0530 Assembling program pass 2 - final. "t4650.htm"{58} I0660 16bit TINY BIN file "t4650.bin" created, size=192. "t4650.htm"{92} I0650 Program "t4650" assembled in 2 passes with errorlevel 0. "t4650.htm"{92} I0750 Source "t4650" (110 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4650.htm.lst" created, size=2233. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲